{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["Vejledning","Ø16 - 50W","Ø20 - 50W","Ø16 - 25W","Ø20 - 25W"],"not_rendered":{"charts":0,"images":7,"macros":1,"external_links":0,"defined_names":4,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Vejledning","index":0,"n_rows":54,"n_cols":21,"rows_kept":54,"cut":false,"hidden":false,"merged":[[32,10,32,20],[33,10,33,20]]}
[null,null,null,null,null,null,"Ø16x2 mm, 50 W/m2"]
[null,null," Forindstillingsberegning til Danfoss gulvvarmemanifold type FHF"]
[null,null,"Installatør:"]
[null,null,"Installationsadrese:"]
[null,null,"Kontaktperson:"]
[null,null,"Postnr. og by:"]
[]
[]
[null,null,"Kreds #","Kreds navn","Kreds længde","Afrunding","Forindstilling"]
[null,null,1,"Køkken",83,{"$f":"MROUND(E10,5)","v":85},{"$f":"IFERROR((INDEX($K$36:$U$54,MATCH(F10,$J$36:$J$54,0),MATCH($K$34,$K$35:$U$35,0))),\"\")","v":"n"}]
[null,null,2,"Stue",58,{"$f":"MROUND(E11,5)","v":60},3.5]
[null,null,3,"Stue 2",52,50,2.5]
[null,null,4,"Entre",11,10,1]
[null,null,5,"Bryggers",14,15,1]
[null,null,6,"Værelse 1",15,15,1]
[null,null,7,"Værelse 2",23,25,1]
[null,null,8,"Værelse 3",37,35,1.5]
[null,null,9,"Kontor",19,20,1]
[null,null,10,"Soveværelse",42,40,2]
[null,null,11,"Bad 1",12,10,1]
[null,null,12,"Bad 2",17,15,1]
[null,null,13,null,null,0,{"$f":"IFERROR((INDEX($K$36:$U$54,MATCH(F22,$J$36:$J$54,0),MATCH($K$34,$K$35:$U$35,0))),\"\")","v":""}]
[null,null,14,null,null,0,{"$f":"IFERROR((INDEX($K$36:$U$54,MATCH(F23,$J$36:$J$54,0),MATCH($K$34,$K$35:$U$35,0))),\"\")","v":""}]
[null,null,15,null,null,0,""]
[null,null,16,null,null,0,""]
[]
[null,null,"Forudsætninger: varmetab 50 W/m2, Δt= 5oC"]
[]
[]
[]
[null,null,"Kommentarer:"]
[]
[null,null,null,null,null,null,null,null,null,null,"Længste kreds"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"LARGE(F10:F25,1)","v":85}]
[null,null,null,null,null,null,null,null,null,null,100,95,90,85,80,75,70,65,60,55,50]
[null,null,null,null,null,null,null,null,null,100,"n","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,95,6,"n","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,90,5,6,"n","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,85,4,5,6,"n","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,80,4,4,5,6,"n","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,75,3.5,3.5,4,4.5,5.5,"n","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,70,3,3.5,3.5,4,4.5,5.5,"n","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,65,3,3,3.5,3.5,4,4.5,5.5,"n","-","-","-"]
[null,null,null,null,null,null,null,null,null,60,2.5,3,3,3.5,3.5,4,45,5.5,"n","-","-"]
[null,null,null,null,null,null,null,null,null,55,2.5,2.5,2.5,3,3,3.5,4,1.5,5.5,"n","-"]
[null,null,null,null,null,null,null,null,null,50,2,2,2.5,2.5,2.5,3,3.5,1,4.5,5.5,"n"]
[null,null,null,null,null,null,null,null,null,45,1.5,1.5,2,2.5,2.5,2.5,3,3.5,3.5,4,5.5]
[null,null,null,null,null,null,null,null,null,40,1,1.5,1.5,2,2,2.5,25,3,3,3.5,4]
[null,null,null,null,null,null,null,null,null,35,1,1,1,1.5,1.5,2,2.5,2.5,2.5,2.5,3.5]
[null,null,null,null,null,null,null,null,null,30,"-",1,1,1,1,1.5,1.5,2,2.5,2,3]
[null,null,null,null,null,null,null,null,null,25,"-",1,1,1,1,1,1,1.5,2,1.5,2.5]
[null,null,null,null,null,null,null,null,null,20,"-",1,1,1,1,1,1,1,1,1,2]
[null,null,null,null,null,null,null,null,null,15,"-",1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,10,"-",1,1,1,1,1,1,1,1,1,1]

{"sheet":"Ø16 - 50W","index":1,"n_rows":54,"n_cols":21,"rows_kept":54,"cut":false,"hidden":false,"merged":[[32,10,32,20],[33,10,33,20],[31,2,36,6]]}
[null,null,null,null,null,null,"Ø16x2 mm, 50 W/m2"]
[null,null," Forindstillingsberegning til Danfoss gulvvarmemanifold type FHF"]
[null,null,"Installatør:"]
[null,null,"Installationsadresse:"]
[null,null,"Kontaktperson:"]
[null,null,"Postnr. og by:"]
[]
[]
[null,null,"Kreds #","Kreds navn","Kreds længde [m]","Afrunding","Forindstilling"]
[null,null,1,null,null,{"$f":"MROUND(E10,5)","v":0},{"$f":"IFERROR((INDEX($K$36:$U$54,MATCH(F10,$J$36:$J$54,0),MATCH($K$34,$K$35:$U$35,0))),\"\")","v":""}]
[null,null,2,null,null,{"$f":"MROUND(E11,5)","v":0},{"$f":"IFERROR((INDEX($K$36:$U$54,MATCH(F11,$J$36:$J$54,0),MATCH($K$34,$K$35:$U$35,0))),\"\")","v":""}]
[null,null,3,null,null,0,{"$f":"IFERROR((INDEX($K$36:$U$54,MATCH(F12,$J$36:$J$54,0),MATCH($K$34,$K$35:$U$35,0))),\"\")","v":""}]
[null,null,4,null,null,0,{"$f":"IFERROR((INDEX($K$36:$U$54,MATCH(F13,$J$36:$J$54,0),MATCH($K$34,$K$35:$U$35,0))),\"\")","v":""}]
[null,null,5,null,null,0,""]
[null,null,6,null,null,0,""]
[null,null,7,null,null,0,{"$f":"IFERROR((INDEX($K$36:$U$54,MATCH(F16,$J$36:$J$54,0),MATCH($K$34,$K$35:$U$35,0))),\"\")","v":""}]
[null,null,8,null,null,0,""]
[null,null,9,null,null,0,""]
[null,null,10,null,null,0,""]
[null,null,11,null,null,0,""]
[null,null,12,null,null,0,""]
[null,null,13,null,null,0,""]
[null,null,14,null,null,0,""]
[null,null,15,null,null,0,""]
[null,null,16,null,null,0,""]
[]
[null,null,"Forudsætninger: varmetab 50 W/m2, Δt= 5oC"]
[]
[null,null,{"$f":"IF(OR(E10>100,E11>100,E12>100,E13>100,E14>100,E15>100,E16>100,E17>100,E18>100,E19>100,E21>100,E20>100,E22>100,E23>100,E24>100,E25>100),\"Max. tryktab overskredet (100 m), reducér kreds længde.\",\"\")","v":""}]
[]
[null,null,"Kommentarer:"]
[]
[null,null,null,null,null,null,null,null,null,null,"Længste kreds"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"LARGE(F10:F25,1)","v":0}]
[null,null,null,null,null,null,null,null,null,null,100,95,90,85,80,75,70,65,60,55,50]
[null,null,null,null,null,null,null,null,null,100,"n","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,95,6,"n","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,90,5,6,"n","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,85,4,5,6,"n","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,80,4,4,5,6,"n","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,75,3.5,3.5,4,4.5,5.5,"n","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,70,3,3.5,3.5,4,4.5,5.5,"n","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,65,3,3,3.5,3.5,4,4.5,5.5,"n","-","-","-"]
[null,null,null,null,null,null,null,null,null,60,2.5,3,3,3.5,3.5,4,45,5.5,"n","-","-"]
[null,null,null,null,null,null,null,null,null,55,2.5,2.5,2.5,3,3,3.5,4,1.5,5.5,"n","-"]
[null,null,null,null,null,null,null,null,null,50,2,2,2.5,2.5,2.5,3,3.5,1,4.5,5.5,"n"]
[null,null,null,null,null,null,null,null,null,45,1.5,1.5,2,2.5,2.5,2.5,3,3.5,3.5,4,5.5]
[null,null,null,null,null,null,null,null,null,40,1,1.5,1.5,2,2,2.5,25,3,3,3.5,4]
[null,null,null,null,null,null,null,null,null,35,1,1,1,1.5,1.5,2,2.5,2.5,2.5,2.5,3.5]
[null,null,null,null,null,null,null,null,null,30,"-",1,1,1,1,1.5,1.5,2,2.5,2,3]
[null,null,null,null,null,null,null,null,null,25,"-",1,1,1,1,1,1,1.5,2,1.5,2.5]
[null,null,null,null,null,null,null,null,null,20,"-",1,1,1,1,1,1,1,1,1,2]
[null,null,null,null,null,null,null,null,null,15,"-",1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,10,"-",1,1,1,1,1,1,1,1,1,1]

{"sheet":"Ø20 - 50W","index":2,"n_rows":58,"n_cols":25,"rows_kept":58,"cut":false,"hidden":false,"merged":[[32,10,32,20],[33,10,33,20],[31,2,36,6]]}
[null,null,null,null,null,null,"Ø20x2 mm, 50 W/m2"]
[null,null," Forindstillingsberegning til Danfoss gulvvarmemanifold type FHF"]
[null,null,"Installatør:"]
[null,null,"Installationsadresse:"]
[null,null,"Kontaktperson:"]
[null,null,"Postnr. og by:"]
[]
[]
[null,null,"Kreds #","Kreds navn","Kreds længde [m]","Afrunding","Forindstilling"]
[null,null,1,null,null,{"$f":"MROUND(E10,5)","v":0},{"$f":"IFERROR((INDEX($K$36:$Y$58,MATCH(F10,$J$36:$J$58,0),MATCH($K$34,$K$35:$Y$35,0))),\"\")","v":""}]
[null,null,2,null,null,{"$f":"MROUND(E11,5)","v":0},{"$f":"IFERROR((INDEX($K$36:$Y$58,MATCH(F11,$J$36:$J$58,0),MATCH($K$34,$K$35:$Y$35,0))),\"\")","v":""}]
[null,null,3,null,null,0,""]
[null,null,4,null,null,0,""]
[null,null,5,null,null,0,""]
[null,null,6,null,null,0,""]
[null,null,7,null,null,0,""]
[null,null,8,null,null,0,""]
[null,null,9,null,null,0,""]
[null,null,10,null,null,0,""]
[null,null,11,null,null,0,""]
[null,null,12,null,null,0,""]
[null,null,13,null,null,0,""]
[null,null,14,null,null,0,""]
[null,null,15,null,null,0,""]
[null,null,16,null,null,0,""]
[]
[null,null,"Forudsætninger: varmetab 50 W/m2, Δt= 5oC"]
[]
[null,null,{"$f":"IF(OR(E10>120,E11>120,E12>120,E13>120,E14>120,E15>120,E16>120,E17>120,E18>120,E19>120,E21>120,E20>120,E22>120,E23>120,E24>120,E25>120),\"Max. tryktab overskredet (120 m), reducér kreds længde.\",\"\")","v":""}]
[]
[null,null,"Kommentarer:"]
[]
[null,null,null,null,null,null,null,null,null,null,"Længste kreds"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"LARGE(F10:F25,1)","v":0}]
[null,null,null,null,null,null,null,null,null,null,120,115,110,105,100,95,90,85,80,75,70,65,60,55,50]
[null,null,null,null,null,null,null,null,null,120,"n","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,115,7,"n","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,110,6,6.5,"n","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,105,5.5,6,7,"n","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,100,5,5.5,6,7,"n","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,95,4.5,5,5.5,6.5,7,"n","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,90,4,4.5,5,5.5,6,7,"n","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,85,4,4,4.5,5,5.5,6,7,"n","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,80,3.5,4,4,4.5,5,5.5,6,7,"n","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,75,3.5,3.5,4,4,",4,5",5,5.5,6,7,"n","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,70,3,3.5,3.5,4,4.5,4.5,5,5.5,6,7,"n","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,65,3,3,3.5,3.5,4,4,4.5,5,5,6,7,"n","-","-","-"]
[null,null,null,null,null,null,null,null,null,60,3,3,3,3.5,3.5,4,4,4.5,4.5,5,6,7,"n","-","-"]
[null,null,null,null,null,null,null,null,null,55,2.5,3,3,3,3.5,3.5,3.5,4,4,4.5,5,6,6.5,"n","-"]
[null,null,null,null,null,null,null,null,null,50,2.5,2.5,2.5,3,3,3,3,3.5,4,4,4.5,5,5.5,6.5,"n"]
[null,null,null,null,null,null,null,null,null,45,2,2.5,2.5,2.5,3,3,3,3,3.5,3.5,4,4.5,4.5,5,6]
[null,null,null,null,null,null,null,null,null,40,2,2,2,2.5,2.5,2.5,2.5,3,3,3.5,3.5,4,4,4.5,5]
[null,null,null,null,null,null,null,null,null,35,1.5,1.5,1.5,2,2,2.5,2.5,2.5,2.5,3,3,3.5,3.5,4,4.5]
[null,null,null,null,null,null,null,null,null,30,1,1,1,1.5,1.5,2,2,2,2.5,2.5,2.5,3,3,3.5,4]
[null,null,null,null,null,null,null,null,null,25,1,1,1,1,1.5,1.5,1.5,1.5,2,2,2.5,2.5,2.5,3,3.5]
[null,null,null,null,null,null,null,null,null,20,1,1,1,1,1,1,1,1,1,1.5,1.5,2,2,2.5,2.5]
[null,null,null,null,null,null,null,null,null,15,1,1,1,1,1,1,1,1,1,1,1,1,1.5,1.5,2]
[null,null,null,null,null,null,null,null,null,10,1,1,1,1,1,1,1,1,1,1,1,1,1,1,1]

{"sheet":"Ø16 - 25W","index":3,"n_rows":58,"n_cols":25,"rows_kept":58,"cut":false,"hidden":false,"merged":[[32,10,32,20],[33,10,33,20],[31,2,36,6]]}
[null,null,null,null,null,null,"Ø16x2 mm, 25 W/m2"]
[null,null," Forindstillingsberegning til Danfoss gulvvarmemanifold type FHF"]
[null,null,"Installatør:"]
[null,null,"Installationsadresse:"]
[null,null,"Kontaktperson:"]
[null,null,"Postnr. og by:"]
[]
[]
[null,null,"Kreds #","Kreds navn","Kreds længde [m]","Afrunding","Forindstilling"]
[null,null,1,null,null,{"$f":"MROUND(E10,5)","v":0},{"$f":"IFERROR((INDEX($K$36:$Y$58,MATCH(F10,$J$36:$J$58,0),MATCH($K$34,$K$35:$Y$35,0))),\"\")","v":""}]
[null,null,2,null,null,{"$f":"MROUND(E11,5)","v":0},{"$f":"IFERROR((INDEX($K$36:$Y$58,MATCH(F11,$J$36:$J$58,0),MATCH($K$34,$K$35:$Y$35,0))),\"\")","v":""}]
[null,null,3,null,null,0,""]
[null,null,4,null,null,0,""]
[null,null,5,null,null,0,""]
[null,null,6,null,null,0,""]
[null,null,7,null,null,0,""]
[null,null,8,null,null,0,""]
[null,null,9,null,null,0,""]
[null,null,10,null,null,0,""]
[null,null,11,null,null,0,""]
[null,null,12,null,null,0,""]
[null,null,13,null,null,0,""]
[null,null,14,null,null,0,""]
[null,null,15,null,null,0,""]
[null,null,16,null,null,0,""]
[]
[null,null,"Forudsætninger: varmetab 25 W/m2, Δt= 5oC"]
[]
[null,null,{"$f":"IF(OR(E10>120,E11>120,E12>120,E13>120,E14>120,E15>120,E16>120,E17>120,E18>120,E19>120,E21>120,E20>120,E22>120,E23>120,E24>120,E25>120),\"Max. tryktab overskredet (120 m), reducér kreds længde.\",\"\")","v":""}]
[]
[null,null,"Kommentarer:"]
[]
[null,null,null,null,null,null,null,null,null,null,"Længste kreds"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"LARGE(F10:F25,1)","v":0}]
[null,null,null,null,null,null,null,null,null,null,120,115,110,105,100,95,90,85,80,75,70,65,60,55,50]
[null,null,null,null,null,null,null,null,null,120,"n","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,115,6,"n","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,110,5,6,"n","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,105,4,5,6,"n","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,100,4,4,5,6,"n","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,95,3.5,4,4,5,6,"n","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,90,3,3.5,4,4,5,6,"n","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,85,3,3,3.5,4,4,5,6,"n","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,80,2.5,3,3,3.5,4,4,5,6,"n","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,75,2.5,2.5,3,3,3.5,3.5,4,4.5,5.5,"n","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,70,2,2.5,2.5,3,3,3.5,3.5,4,4.5,5.5,"n","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,65,1.5,2,2.5,2.5,3,3,3.5,3.5,4,4.5,5.5,"n","-","-","-"]
[null,null,null,null,null,null,null,null,null,60,1,1.5,2,2.5,2.5,3,3,3.5,3.5,4,4.5,5.5,"n","-","-"]
[null,null,null,null,null,null,null,null,null,55,1,1,1.5,2,2.5,2.5,2.5,3,3,3.5,4,1.5,5.5,"n","-"]
[null,null,null,null,null,null,null,null,null,50,1,1,1,1.5,2,2,2.5,2.5,2.5,3,3.5,1,4.5,5.5,"n"]
[null,null,null,null,null,null,null,null,null,45,"-",1,1,1,1.5,1.5,2,2.5,2.5,2.5,3,3.5,3.5,4,5.5]
[null,null,null,null,null,null,null,null,null,40,"-",1,1,1,1,1.5,1.5,2,2,2.5,2.5,3,3,3.5,4]
[null,null,null,null,null,null,null,null,null,35,"-","-",1,1,1,1,1,1.5,1.5,2,2.5,2.5,2.5,2.5,3.5]
[null,null,null,null,null,null,null,null,null,30,"-","-",1,1,1,1,1,1,1,1.5,1.5,2,2.5,2,3]
[null,null,null,null,null,null,null,null,null,25,"-","-","-",1,1,1,1,1,1,1,1,1.5,2,1.5,2.5]
[null,null,null,null,null,null,null,null,null,20,"-","-","-",1,1,1,1,1,1,1,1,1,1,1,2]
[null,null,null,null,null,null,null,null,null,15,"-","-","-","-",1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,10,"-","-","-","-",1,1,1,1,1,1,1,1,1,1,1]

{"sheet":"Ø20 - 25W","index":4,"n_rows":64,"n_cols":25,"rows_kept":64,"cut":false,"hidden":false,"merged":[[32,10,32,20],[33,10,33,20],[31,2,36,6]]}
[null,null,null,null,null,null,"Ø20x2 mm, 25 W/m2"]
[null,null," Forindstillingsberegning til Danfoss gulvvarmemanifold type FHF"]
[null,null,"Installatør:"]
[null,null,"Installationsadresse:"]
[null,null,"Kontaktperson:"]
[null,null,"Postnr. og by:"]
[]
[]
[null,null,"Kreds #","Kreds navn","Kreds længde [m]","Afrunding","Forindstilling"]
[null,null,1,null,null,{"$f":"MROUND(E10,5)","v":0},{"$f":"IFERROR((INDEX($K$36:$Y$64,MATCH(F10,$J$36:$J$64,0),MATCH($K$34,$K$35:$Y$35,0))),\"\")","v":""}]
[null,null,2,null,null,{"$f":"MROUND(E11,5)","v":0},{"$f":"IFERROR((INDEX($K$36:$Y$64,MATCH(F11,$J$36:$J$64,0),MATCH($K$34,$K$35:$Y$35,0))),\"\")","v":""}]
[null,null,3,null,null,0,""]
[null,null,4,null,null,0,""]
[null,null,5,null,null,0,""]
[null,null,6,null,null,0,""]
[null,null,7,null,null,0,""]
[null,null,8,null,null,0,""]
[null,null,9,null,null,0,""]
[null,null,10,null,null,0,""]
[null,null,11,null,null,0,""]
[null,null,12,null,null,0,""]
[null,null,13,null,null,0,""]
[null,null,14,null,null,0,""]
[null,null,15,null,null,0,""]
[null,null,16,null,null,0,""]
[]
[null,null,"Forudsætninger: varmetab 25 W/m2, Δt= 5oC"]
[]
[null,null,{"$f":"IF(OR(E10>150,E11>150,E12>150,E13>150,E14>150,E15>150,E16>150,E17>150,E18>150,E19>150,E21>150,E20>150,E22>150,E23>150,E24>150,E25>150),\"Max. tryktab overskredet (150 m), reducér kreds længde.\",\"\")","v":""}]
[]
[null,null,"Kommentarer:"]
[]
[null,null,null,null,null,null,null,null,null,null,"Længste kreds"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"LARGE(F10:F25,1)","v":0}]
[null,null,null,null,null,null,null,null,null,null,150,145,140,135,130,125,120,115,110,105,100,95,90,85,80]
[null,null,null,null,null,null,null,null,null,150,"n","-","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,145,7,"n","-","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,140,6,7,"n","-","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,135,5.5,6,7,"n","-","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,130,5,5.5,6,7,"n","-","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,125,4.5,5,5.5,6,7,"n","-","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,120,4,4.5,5,5.5,6,7,"n","-","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,115,4,4,4.5,5,5.5,6,7,"n","-","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,110,3.5,4,4,4.5,5,5.5,6,6.5,"n","-","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,105,3.5,3.5,4,4,4.5,5,5.5,6,7,"n","-","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,100,3,3.5,3.5,4,4,4.5,5,5.5,6,7,"n","-","-","-","-"]
[null,null,null,null,null,null,null,null,null,95,3,3,3.5,3.5,4,4,4.5,5,5.5,6.5,7,"n","-","-","-"]
[null,null,null,null,null,null,null,null,null,90,3,3,3,3.5,3.5,4,4,4.5,5,5.5,6,7,"n","-","-"]
[null,null,null,null,null,null,null,null,null,85,2.5,3,3,3,3.5,3.5,4,4,4.5,5,5.5,6,7,"n","-"]
[null,null,null,null,null,null,null,null,null,80,2.5,2.5,3,3,3,3.5,3.5,4,4,4.5,5,5.5,6,7,"n"]
[null,null,null,null,null,null,null,null,null,75,2,2.5,2.5,3,3,3,3.5,3.5,4,4,4.5,5,5.5,6,7]
[null,null,null,null,null,null,null,null,null,70,2,2,2.5,2.5,3,3,3,3.5,3.5,4,4.5,4.5,5,5.5,6]
[null,null,null,null,null,null,null,null,null,65,1.5,2,2,2.5,2.5,3,3,3,3.5,3.5,4,4,4.5,5,5]
[null,null,null,null,null,null,null,null,null,60,1,1.5,2,2,2.5,2.5,3,3,3,3.5,3.5,4,4,4.5,4.5]
[null,null,null,null,null,null,null,null,null,55,1,1,1.5,2,2,2.5,2.5,3,3,3,3.5,3.5,3.5,4,4]
[null,null,null,null,null,null,null,null,null,50,1,1,1,1.5,2,2,2.5,2.5,2.5,3,3,3,3,3.5,4]
[null,null,null,null,null,null,null,null,null,45,1,1,1,1,1.5,2,2,2.5,2.5,2.5,3,3,3,3,3.5]
[null,null,null,null,null,null,null,null,null,40,1,1,1,1,1,1.5,2,2,2,2.5,2.5,2.5,2.5,3,3]
[null,null,null,null,null,null,null,null,null,35,1,1,1,1,1,1,1.5,1.5,1.5,2,2,2.5,2.5,2.5,2.5]
[null,null,null,null,null,null,null,null,null,30,"-",1,1,1,1,1,1,1,1,1.5,1.5,2,2,2,2.5]
[null,null,null,null,null,null,null,null,null,25,"-","-",1,1,1,1,1,1,1,1,1.5,1.5,1.5,1.5,2]
[null,null,null,null,null,null,null,null,null,20,"-","-","-",1,1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,15,"-","-","-","-",1,1,1,1,1,1,1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,10,"-","-","-","-","-",1,1,1,1,1,1,1,1,1,1]